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MATERIAL SAFETY DATA SHEET
ANISOLE 
(For Synthesis)
MSDS CAS: 100-66-3
	Section 1: Chemical Product and Company Identification



Section 1: Chemical Product 
Product Name:Anisole
CAS#:  100-66-3
C.I. No.:Not available.
Synonym: Methoxybenzene
Chemical Name:Not available.
Chemical Formula:C7H8O

Brand: OXFORD
Details Of The Supplier Of The Safety Data Sheet:
Company identification:   OXFORD LAB FINE CHEM LLP
				    Unit. No. 12, 1st Floor, Neminath Industrial Estate No. 6,
                                             Navghar, Vasai (East). Palghar - 401 210.
				    Mumbai, Maharashtra, INDIA.
				    Tel: 91-250-2390989
				    Tel/Fax:  91-250-2390032

	Section 2: Composition and Information on Ingredients



Composition:

	Name
	CAS #
	% by Weight

	Anisole
	100-66-3
	100



Toxicological Data on Ingredients: Anisole: ORAL (LD50): Acute: 3700 mg/kg [Rat]. 2800 mg/kg [Mouse].
	Section 3: Hazards Identification



Potential Acute Health Effects: Hazardous in case of skin contact (irritant), of eye contact (irritant), of ingestion, of inhalation.

Potential Chronic Health Effects: Hazardous in case of skin contact (irritant), of eye contact (irritant), of ingestion, of inhalation. CARCINOGENIC EFFECTS:Not available. MUTAGENIC EFFECTS: Not available. TERATOGENIC EFFECTS: Not available. DEVELOPMENTALTOXICITY: Not available.

	Section 4: First Aid Measures



Eye Contact:
Check for and remove any contact lenses. In case of contact, immediately flush eyes with plenty of water for at least 15 minutes. Get medical attention.
Skin Contact:
In case of contact, immediately flush skin with plenty of water. Cover the irritated skin with an emollient. Remove contaminated clothing and shoes. Wash clothing before reuse. Thoroughly clean shoes before reuse. Get medical attention.
Serious Skin Contact:
Wash with a disinfectant soap and cover the contaminated skin with an anti-bacterial cream. Seek medical attention.
Inhalation:
If inhaled, remove to fresh air. If not breathing, give artificial respiration. If breathing is difficult, give oxygen. Get medical attention if symptoms appear.
Serious Inhalation:
Evacuate the victim to a safe area as soon as possible. Loosen tight clothing such as a collar, tie, belt or waistband. If breathing is difficult, administer oxygen. If the victim is not breathing, perform mouth-to-mouth resuscitation. Seek medical attention.
Ingestion:
Do NOT induce vomiting unless directed to do so by medical personnel. Never give anything by mouth to an unconscious person. Loosen tight clothing such as a collar, tie, belt or waistband. Get medical attention if symptoms appear.
Serious Ingestion: Not available.

	Section 5: Fire and Explosion Data



Flammability of the Product: Flammable.
Auto-Ignition Temperature: 475°C (887°F)
Flash Points: CLOSED CUP: 83°C (181.4°F). OPEN CUP: 52°C (125.6°F).
	Section 5: Fire and Explosion Data(Continued)



Flammable Limits: LOWER: 0.3% UPPER: 6.3%
Products of Combustion: These products are carbon oxides (CO, CO2).
Fire Hazards in Presence of Various Substances: Flammable in presence of open flames and sparks, of heat.
Explosion Hazards in Presence of Various Substances:
Risks of explosion of the product in presence of mechanical impact: Not available. Risks of explosion of the product in
presence of static discharge: Not available.
Fire Fighting Media and Instructions:
Flammable liquid, insoluble in water. SMALL FIRE: Use DRY chemical powder. LARGE FIRE: Use water spray or fog. Cool
containing vessels with water jet in order to prevent pressure build-up, autoignition or explosion.
Special Remarks on Fire Hazards: Not available.
Special Remarks on Explosion Hazards:Not available.

	Section 6: Accidental Release Measures



Small Spill: Absorb with an inert material and put the spilled material in an appropriate waste disposal.

Large Spill:
Flammable liquid, insoluble in water. Keep away from heat. Keep away from sources of ignition. Stop leak if without risk. Absorb with DRY earth, sand or other non-combustible material. Do not get water inside container. Do not touch spilled material. Prevent entry into sewers, basements or confined areas; dike if needed. Call for assistance on disposal.

	Section 7: Handling and Storage



Precautions:
Keep away from heat. Keep away from sources of ignition. Ground all equipment containing material. Do not ingest. Do notbreathe gas/fumes/ vapor/spray. Wear suitable protective clothing. In case of insufficient ventilation, wear suitable respiratory equipment. If ingested, seek medical advice immediately and show the container or the label. Avoid contact with skin and eyes.

Storage:
Store in a segregated and approved area. Keep container in a cool, well-ventilated area. Keep container tightly closed and sealed until ready for use. Avoid all possible sources of ignition (spark or flame).

	Section 8: Exposure Controls/Personal Protection



Engineering Controls:
Provide exhaust ventilation or other engineering controls to keep the airborne concentrations of vapors below their respective threshold limit value. Ensure that eyewash stations and safety showers are proximal to the work-station location.
Personal Protection:
Splash goggles. Lab coat. Vapor respirator. Be sure to use an approved/certified respirator or equivalent. Gloves.
Personal Protection in Case of a Large Spill:
Splash goggles. Full suit. Vapor respirator. Boots. Gloves. A self contained breathing apparatus should be used to avoid inhalation of the product. Suggested protective clothing might not be sufficient; consult a specialist BEFORE handling this product.
Exposure Limits: Not available.

	Section 9: Physical and Chemical Properties



Physical state and appearance: Liquid.
Odor:Sweet anise-like odor
Taste                                                                            : Not available.
Molecular Weight                                                       : 108.13 g/mole
Color                                                                            : Clear colorless.
pH (1% soln/water): Not applicable.	
Boiling Point                                                               : 155.5°C (311.9°F)
Melting Point: -37.3°C (-35.1°F)
Critical Temperature: Not available.
Specific Gravity:0.9956 (Water = 1)
Vapor Pressure: Not available.
Vapor Density: 3.72 (Air = 1)
Volatility: Not available.
Odor Threshold: Not available.
Water/Oil Dist. Coeff.                                                 : Not available.
Ionicity (in Water): Not available.
Dispersion Properties: See solubility in water, methanol, acetone.
[bookmark: _GoBack]Solubility: Soluble in methanol, acetone. Insoluble in cold water.


	Section 10: Stability and Reactivity Data



Stability:The product is stable.
Instability Temperature: Not available.
Conditions of Instability: Not available.
Incompatibility with various substances: Not available.
Corrosivity: Non-corrosive in presence of glass.
Special Remarks on Reactivity: Not available.
Special Remarks on Corrosivity: Not available.
Polymerization: Will not occur.

	Section 11: Toxicological Information



Routes of Entry: Eye contact. Inhalation. Ingestion.
Toxicity to Animals: WARNING: THE LC50 VALUES HEREUNDER ARE ESTIMATED ON THE BASIS OF A 4-HOUR EXPOSURE. Acute oraltoxicity (LD50): 2800 mg/kg [Mouse]. Acute toxicity of the vapor (LC50): 5001 8 hours [Rat].
Chronic Effects on Humans: Not available.
Other Toxic Effects on Humans: Hazardous in case of skin contact (irritant), of ingestion, of inhalation.
Special Remarks on Toxicity to Animals: Not available.
Special Remarks on Chronic Effects on Humans: Not available.
Special Remarks on other Toxic Effects on Humans: Not available.
	Section 12: Ecological Information



Ecotoxicity:Not available.
BOD5 and COD:Not available.
Products of Biodegradation: Possibly hazardous short term degradation products are not likely. However, long term degradation products may arise.
Toxicity of the Products ofBiodegradation:The products of degradation are more toxic.
Special Remarks on the Products of Biodegradation:Not available.

	Section 13: Disposal Considerations



Waste Disposal:

	Section 14: Transport Information



14.1. Land transport (ADR-RID)

Proper shipping name 			: ANISOLE
UN N° 					: 2222
H.I. nr 					: 30
ADR - Class 					: 6.1
Labelling - Transport 			: 3 :Flamabble Liquid
ADR – Group				: III

14.2. Sea transport (IMDG) [English only]

Proper shipping name			: ANISOLE
UN N°					: 2222
IMO-IMDG - Class or division	: 3 :Flamabble Liquid
IMO-IMDG - Packing group		: III

14.3. Air transport (ICAO-IATA) [English only]

Proper shipping name			: ANISOLE
UN N°					: 2222
IMO-IMDG - Class or division	: 3 :Flamabble Liquid
IMO-IMDG - Packing group		: III

	Section 15: Other Regulatory Information



Federal and State Regulations: TSCA 8(b) inventory: Anisole
Other Regulations: OSHA: Hazardous by definition of Hazard Communication Standard (29 CFR 1910.1200).
Other Classifications:
WHMIS (Canada): CLASS B-2: Flammable liquid with a flash point lower than 37.8°C (100°F).
DSCL (EEC): R36/38- Irritating to eyes and skin.
HMIS (U.S.A.):
Health Hazard: 1
Fire Hazard:2
Reactivity: 0

Personal Protection: h
National Fire Protection Association (U.S.A.):
Health: 1
Flammability: 2
Reactivity: 0
Specific hazard:
Protective Equipment: Gloves. Lab coat. Vapor respirator. Be sure to use an approved/certified respirator or equivalent. Wear appropriate respirator when ventilation is inadequate. Splash goggles.
	Section 15: Other Regulatory Information(Continued)



	Section 16 - Additional Information



References: Not available.
Other Special Considerations: Not available.
Disclaimer:
**************************************************************************************************************************
The information contained herein in good faith but makes no representations as to its comprehensiveness or accuracy. This document is intended only as a guide to the appropriate precautionary handling of the material by a properly trained person using this product. Individuals receiving the information must exercise their independent judgment in determining its appropriateness for a particular purpose.	
Oxford Lab Fine ChemLLP makes no representations or warranties, either express or implied, including without limitation any warranties of merchantability, fitness for a particular purpose with respect to the information set forth herein or the product to which the information refers. Accordingly, Oxford Lab Fine Chem LLP will not be responsible for damages resulting from use of or reliance upon this information.
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