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MATERIAL SAFETY DATA SHEET
CHROMIUM METAL POWDER 99%
(Extra Pure)
MSDS CAS: 7440-47-3
	Section 1: Chemical Product and Company Identification



Section 1: Chemical Product 
Product Name: CHROMIUM METAL POWDER
CAS#:   7440-47-3
Synonym: Chromium metal; Chrome; Chromium Metal
Chips 2" and finer
Chemical Name: Chromium Metal Lumps
Chemical Formula:  Cr


Brand : OXFORD
Details Of The Supplier Of The Safety Data Sheet :
Company identification:      OXFORD LAB FINE CHEM LLP
				       Unit. No. 12, 1st Floor, Neminath Industrial Estate No. 6,
                                                Navghar, Vasai (East). Palghar - 401 210.
				       Mumbai, Maharashtra, INDIA.
				       Tel: 91-250-2390989
				       Tel/Fax:  91-250-2390032

	Section 2: Composition and Information on Ingredients



Composition:
	Name
	CAS #
	% by Weight

	Chromium Metal Powder
	7440-47-3
	100



Toxicological Data on Ingredients:  Chromium Metal Powder LD50: Not available. LC50: Not available.
	Section 3: Hazards Identification



Potential Acute Health Effects: 
Hazardous in case of skin contact (irritant), of eye contact (irritant), of inhalation. Slightly hazardous in case of ingestion.

Potential Chronic Health Effects:
CARCINOGENIC EFFECTS: A4 (Not classifiable for human or animal.) by ACGIH, 3 (Not classifiable for human.) by IARC.
MUTAGENIC EFFECTS: Not available. 
TERATOGENIC EFFECTS: Not available.
DEVELOPMENTAL TOXICITY: Not available. 
The substance may be toxic to kidneys, lungs, liver, upper respiratory tract. Repeated or prolonged exposure to the substance can produce target organs damage.

	Section 4: First Aid Measures



Eye Contact:  
Check for and remove any contact lenses. In case of contact, immediately flush eyes with plenty of water for at least 15 minutes. Get medical attention.

Skin Contact: 
In case of contact, immediately flush skin with plenty of water. Cover the irritated skin with an emollient. Remove contaminated clothing and shoes. Wash clothing before reuse. Thoroughly clean shoes before reuse. Get medical attention.

Serious Skin Contact:  
Wash with a disinfectant soap and cover the contaminated skin with an anti-bacterial cream. Seek medical attention.

Inhalation:  
If inhaled, remove to fresh air. If not breathing, give artificial respiration. If breathing is difficult, give oxygen. Get medical attention.

Serious Inhalation:  Not available.
 
Ingestion:
Do NOT induce vomiting unless directed to do so by medical personnel. Never give anything by mouth to an unconscious person. Loosen tight clothing such as a collar, tie, belt or waistband. Get medical attention if symptoms appear.

Serious Ingestion: Not available.
	Section 5: Fire and Explosion Data



Flammability of the Product: May be combustible at high temperature.
 
Auto-Ignition Temperature: 580°C (1076°F)

Flash Points: Not available.

Flammable Limits: Not available.

Products of Combustion:  Some metallic oxides.

Fire Hazards in Presence of Various Substances: 
Slightly flammable to flammable in presence of open flames and sparks, of heat. Non-flammable in presence of shocks.

Explosion Hazards in Presence of Various Substances:  
Risks of explosion of the product in presence of mechanical impact: Not available. 
Risks of explosion of the product in presence of static discharge: Not available.

Fire Fighting Media and Instructions:  
SMALL FIRE: Use DRY chemical powder. 
LARGE FIRE: Use water spray, fog or foam. Do not use water jet.

Special Remarks on Fire Hazards: 
Moderate fire hazard when it is in the form of a dust (powder) and burns rapidly when heated in flame. Chromium is attacked vigorously by fused potassium chlorate producing vivid incandescence. Pyrophoric chromium unites with nitric oxide with incandescence. Incandescent reaction with nitrogen oxide or sulfur dioxide.

Special Remarks on Explosion Hazards: 
Powdered Chromium metal +fused ammonium nitrate may react violently or explosively. Powdered Chromium will explode spontaneously in air.

	Section 6: Accidental Release Measures



Small Spill:  
Use appropriate tools to put the spilled solid in a convenient waste disposal container. Finish cleaning by spreading water on the contaminated surface and dispose of according to local and regional authority requirements.
	Section 6: Accidental Release Measures (Continued)



Large Spill:
Use a shovel to put the material into a convenient waste disposal container. Finish cleaning by spreading water on the contaminated surface and allow to evacuate through the sanitary system. Be careful that the product is not present at a concentration level above TLV. Check TLV on the MSDS and with local authorities.

	Section 7: Handling and Storage



Precautions:
Keep away from heat. Keep away from sources of ignition. Ground all equipment containing material. Do not ingest. Do not breathe dust. Wear suitable protective clothing. In case of insufficient ventilation, wear suitable respiratory equipment. If ingested, seek medical advice immediately and show the container or the label. Avoid contact with skin and eyes. Keep away from incompatibles such as oxidizing agents, acids, alkalis.

Storage: 
Keep container tightly closed. Keep container in a cool, well-ventilated area.

	Section 8: Exposure Controls/Personal Protection



Engineering Controls:
Use process enclosures, local exhaust ventilation, or other engineering controls to keep airborne levels below recommended exposure limits. If user operations generate dust, fume or mist, use ventilation to keep exposure to airborne contaminants below the exposure limit.

Personal Protection:  
Splash goggles. Lab coat. Dust respirator. Be sure to use an approved/certified respirator or equivalent. Gloves.
	
Personal Protection in Case of a Large Spill:
Splash goggles. Full suit. Dust respirator. Boots. Gloves. A self contained breathing apparatus should be used to avoid inhalation of the product. Suggested protective clothing might not be sufficient; consult a specialist BEFORE handling this product.

Exposure Limits:  
TWA: 0.5 (mg/m3) from ACGIH (TLV) [United States] TWA: 1 (mg/m3) from OSHA (PEL) [United States] TWA: 0.5 (mg/m3) from NIOSH [United States] TWA: 0.5 (mg/m3) [United Kingdom (UK)] TWA: 0.5 (mg/m3) [Canada] Consult local authorities for acceptable exposure limits.
	Section 9: Physical and Chemical Properties



Physical state and appearance: Solid. 
Odor					: Odorless.
Taste					: Not available.
Molecular Weight		: 52 g/mole
Color					: Bright grey.
pH (1% soln/water)		: Not applicable.
Boiling Point		: 2642°C (4787.6°F)
[bookmark: _GoBack]Melting Point		: 1900°C (3452°F) +/- !0 deg. C
Critical Temperature		: Not available.
Specific Gravity			: 7.14 (Water = 1)
Vapor Pressure			: Not applicable.
Vapor Density			: Not applicable.
Volatility				: Not available.
Odor Threshold			: Not applicable.
Water/Oil Dist. Coeff.		: Not applicable.
Ionicity (in Water)		: Not available.
Dispersion Properties		: Not available.
Solubility	                    		: Insoluble in cold water, hot water. Soluble in acids (except Nitric), and strong alkalis.
	Section 10: Stability and Reactivity Data




Stability: The product is stable.

Instability Temperature: Not available. 

Conditions of Instability: Excess heat, incompatible materials.

Incompatibility with various substances: 
Reactive with oxidizing agents, acids, alkalis.

Corrosivity:  Not available.
 



	Section 10: Stability and Reactivity Data (Continued)



Special Remarks on Reactivity:  
Incompatible with molten Lithium at 180 deg. C, hydrogen peroxide, hydrochloric acid, sulfuric acid, most caustic alkalis and alkali carbonates, potassium chlorate, sulfur dioxide, nitrogen oxide, bromine pentafluoride. It may react violently or ignite with bromine pentafluoride. Chromium is rapidly attacked by fused sodium hydroxide + potassium nitrate. Potentially hazardous incompatibility with strong oxidizers.

Special Remarks on Corrosivity: Not available.

Polymerization: Will not occur.

	Section 11: Toxicological Information



Routes of Entry:  Inhalation. Ingestion.

Toxicity to Animals:  LD50: Not available. LC50: Not available.

Chronic Effects on Humans:  
CARCINOGENIC EFFECTS: A4 (Not classifiable for human or animal.) by ACGIH, 3 (Not classifiable for human.) by IARC. May cause damage to the following organs: kidneys, lungs, liver, upper respiratory tract.

Other Toxic Effects on Humans:  
Hazardous in case of skin contact (irritant), of inhalation. Slightly hazardous in case of ingestion.

Special Remarks on Toxicity to Animals: Not available.

Special Remarks on Chronic Effects on Humans:  
May cause cancer based on animal data. There is no evidence that exposure to trivalent chromium causes cancer in man.

Special Remarks on other Toxic Effects on Humans:  
Acute Potential Health Effects: May cause skin irritation. Eyes: May cause mechanical eye irritation. Inhalation: May cause irritation of the respiratory tract and mucous membranes of the respiratory tract. Ingestion: May cause gastrointestinal tract irritation with nausea, vomiting, diarrhea. Chronic Potential Health Effects: Inhalation: The effects of chronic exposure include irritation , sneezing, redness of the throat, bronchospasm, asthma, cough, polyps, chronic inflammation, emphysema, chronic bronchitis, pharyngitis, bronchopneumonia, pneumoconiosis. Effects on the nose from chronic chromium exposure include irritation, ulceration, and perforation of the nasal septum. Inflammation and ulceration of the larynx may also occur. Ingestion or Inhalation: Chronic exposure may cause liver and kidney damage.

	Section 12: Ecological Information



Ecotoxicity: Not available.

BOD5 and COD: Not available.
 
Products of Biodegradation:
Possibly hazardous short term degradation products are not likely. However, long term degradation products may arise.

Toxicity of the Products of Biodegradation: 
The product itself and its products of degradation are not toxic.

Special Remarks on the Products of Biodegradation: Not available.

	Section 13: Disposal Considerations




Waste Disposal :
Waste must be disposed of in accordance with federal, state and local environmental control regulations.


	Section 14: Transport Information




Land transport (ADR-RID)

General information : Not regulated.

Sea transport (IMDG) [English only]

General information : Not regulated.

Air transport (ICAO-IATA) [English only]

General information : Not regulated.



	Section 15: Other Regulatory Information



Federal and State Regulations:  
Connecticut hazardous material survey.: Chromium Illinois toxic substances disclosure to employee act: Chromium Illinois chemical safety act: Chromium New York release reporting list: Chromium Rhode Island RTK hazardous substances: Chromium Pennsylvania RTK: Chromium Minnesota: Chromium Michigan critical material: Chromium Massachusetts RTK: Chromium Massachusetts spill list: Chromium New Jersey: Chromium New Jersey spill list: Chromium Louisiana spill reporting: Chromium California Director's List of Hazardous Substances: Chromium TSCA 8(b) inventory: Chromium SARA 313 toxic chemical notification and release reporting: Chromium CERCLA: Hazardous substances.: Chromium: 5000 lbs. (2268 kg).

Other Regulations:   
OSHA: Hazardous by definition of Hazard Communication Standard (29 CFR 1910.1200). EINECS: This product is on the European Inventory of Existing Commercial Chemical Substances.
Other Classifications:
WHMIS (Canada): Not controlled under WHMIS (Canada).
DSCL (EEC): R40- Limited evidence of carcinogenic effect S36/37/39- Wear suitable protective clothing, gloves and eye/face protection. S45- In case of accident or if you feel unwell, seek medical advice immediately (show the label where possible).
HMIS (U.S.A.):
Health Hazard: 2
Fire Hazard: 1
Reactivity: 0
Personal Protection: E

National Fire Protection Association (U.S.A.):
Health: 2
Flammability: 1
Reactivity: 0
Specific hazard:

Protective Equipment: 
Gloves. Lab coat. Dust respirator. Be sure to use an approved/certified respirator or equivalent. Splash goggles.


	Section 16 - Additional Information



References: Not available.
Other Special Considerations: Not available.

Disclaimer:
**************************************************************************************************************************
The information contained herein in good faith but makes no representations as to its comprehensiveness or accuracy. This document is intended only as a guide to the appropriate precautionary handling of the material by a properly trained person using this product. Individuals receiving the information must exercise their independent judgment in determining its appropriateness for a particular purpose.	
Oxford Lab Fine Chem LLP makes no representations or warranties, either express or implied, including without limitation any warranties of merchantability, fitness for a particular purpose with respect to the information set forth herein or the product to which the information refers. Accordingly, Oxford Lab Fine Chem LLP will not be responsible for damages resulting from use of or reliance upon this information.
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